# Viewing SSH Sessions information using EDM

Use the following procedure to display currently active SSH sessions.

## Prerequisites

- Open one of the supported browsers.

- Enter the IP address of the switch to open an EDM session.

## Procedure steps

1. From the navigation tree, double-click Security.

2. In the Security tree, double-click SSH.

3. In the work area, click the SSH Sessions tab.

## Variable definitions

Use the data in the following table to configure an SSH Session.

Variable | Value
--- | ---
SshSessionInetAddressType | Indicates the type of IP address of the SSH client that opened the SSH session.
SshSessionInetAddress | Indicates the IP address of the SSH client that opened the SSH session.