# NNSSndSeqParam

## Definition

      #include <nnsys/snd.h>

      typedef struct NNSSndSeqParam
      {
      u16 bankNo;
      u8 volume;
      u8  channelPrio;
      u8  playerPrio;
      u8  playerNo;
      u16 reserved;
      } NNSSndSeqParam;

## Elements

`bankNo` | Bank number.
`volume` | The initial volume setting.
`channelPrio` | The sound priority.
`playerPrio` | This is the player priority.
`playerNo` | The Player number.
`reserved` | The reserved region.

## Description

The sequence parameter structure. This stores the parameter to be set when the sequence is played.

This structure can be obtained by using either the `NNS_SndArcGetSeqParam` function or the `NNS_SndArcGetSeqArcParam` function.

## See Also

`NNS_SndArcGetSeqParam, NNS_SndArcGetSeqArcParam`

## Revision History

06/01/2004 Initial version.