# NNS_G3dGeIsBufferOK

## C Specification

      #include <nnsys/g3d/gecom.h>

      BOOL
      NNS_G3dGeIsBufferOK(
      u32 numWord);
      );

## Arguments

numWord | The number of data that were appended to the command buffer.

## Return Values

Returns `TRUE` if the data in numWord can be added to the geometry command buffer.

## Description

This function checks whether a `numWord quantity of data can be buffered to the geometry command buffer. Always returns FALSE when the geometry command buffer is not set.`

## See Also

## Revision History

10/15/2004 Revised description.
08/02/2004 Initial version.