# NNS_G3dGeIsSendDLBusy

## C Specification

      #include <nnsys/g3d/gecom.h>

      BOOL NNS_G3dGeIsSendDLBusy(void);

## Arguments

None.

## Return Values

Returns TRUE during DMA transfer of geometry command. Otherwise returns FALSE.

## Description

Returns TRUE when DMA transfer of the geometry command via the `NNS_G3dGeSendDL` function is in the process of being carried out.

## See Also

`NNS_G3dGeWaitSendDL, NNS_G3dGeSendDL`

## Revision History

10/15/2004 Revised description.
08/02/2004 Initial version.