# MO_GetOptimalITCMSize

## C Specification

  `#include <nitro/mobiclip.h>`
  `u32 MO_GetOptimalITCMSize ( void );`

## Description

Retrieve the quantity in bytes of ITCM needed by Mobiclip to achieve optimal playback performance.
This function is used for the code relocation management.

## Arguments

None.

## Return Values

Size in bytes of the desired ITCM quantity.

## See Also

`MO_GetOptimalDTCMSize`
`MO_InitITCMArea`
`MO_InitDTCMArea`

## Revision History

03/03/2008 Initial Version