# MB_DisconnectChild

## C Specification

      #include <nitro/mb.h>

      void MB_DisconnectChild( u16 aid );

## Description

This function operates from the parent side, forcibly disconnecting a child from the MB parent. This function immediately removes control of the DS device as a multiboot child and begins the wireless disconnection process.

This function does not return a callback at the end of the wireless disconnection.

## Arguments

`aid` | The `aid` of the child to disconnect.

## Return Values

None.

## See Also

`None.`

## Revision History

11/10/2004 Initial version