# MI_GetCartridgeRamCycle

## C Specification

  `#include <nitro/mi.h>`
  `MICartridgeRamCycle MI_GetCartridgeRamCycle( void )`

## Description

Gets the cycle value set for accessing the Game Pak's RAM region.

The returned values are in the form of `MICartridgeRamCycle`. The meanings are shown below.

`MI_CTRDG_RAMCYCLE_6` | 6 cycles
`MI_CTRDG_RAMCYCLE_8` | 8 cycles
`MI_CTRDG_RAMCYCLE_10` | 10 cycles
`MI_CTRDG_RAMCYCLE_18` | 18 cycles

## Arguments

None.

## Return Values

The cycle that has been set for accessing the Game Pak's RAM region.

## Internal Operation

Accesses the `EXMEMCNT` I/O register `(0x4000204)`.

## See Also

`MI_SetCartridgeRamCycle, MI_GetCartridgeRomCycle1st, MI_GetCartridgeRomCycle2nd
`

## Revision History

05/25/2004 Name changed by adding "cartridge"
12/18/2003 Initial version