# CARD_THREAD_PRIORITY_DEFAULT

## C Specification

      #include <nitro/card.h>

      #define	CARD_THREAD_PRIORITY_DEFAULT	4

## Description

The constant shows the initial priority value of the CARD asynchronous process thread.
To change the priority of this thread, use the `CARD_SetThreadPriority` function.
For details on the CARD asynchronous process thread, see the explanation of the `CARD_GetThreadPriority` function.

## See Also

`CARD_GetThreadPriority, CARD_SetThreadPriority`

## Revision History

07/28/2004 Initial version