# GX_Init

## C Specification

      #include <nitro/gx/gx.h>

      void GX_Init(void);

## Description

In the graphics register, this function initializes all registers that are not 3D related.

Internally, `GX_SetPower` (`GX_POWER_ALL`) is called.

The GX function uses DAM 3 by default. To change the DMA number, use either the `GX_InitEx` or `GX_SetDefaultDMA` function.

## Arguments

None

## Return Values

None

## See Also

`G3X_Init`, `G3X_Reset`, `G3X_InitTable, `GX_InitEx``

## Revision History

02/09/2004 Changed so that `GX_SetPower` is called internally
01/19/2004 Initial Version