# GX_InitEx

## C Specification

      #include <nitro/gx/gx.h>

      void GX_InitEx( u32 dma_no );

## Description

In the graphics register, this function initializes all registers that are not 3D-related.

Internally, `GX_SetPower` (`GX_POWER_ALL`) is called.

The GX function uses DAM 3 by default, but you can specify the DMA number to use in the GX function. Or, you can specify `GX_DMA_NOT_USE` in the argument to not use the DMA.

## Argument

`dma_no` | Specify the DMA number to use with GX

## Return Values

None

## See Also

`GX_Init, G3X_Init, G3X_Reset, G3X_InitTable`

## Revision History

07/28/2004 Initial version