# CTRDG_TerminateForPulledOut

## C Specification

      #include <nitro/ctrdg.h>

      void CTRDG_TerminateForPulledOut( void );

## Description

This function stops the ARM7 processor and the program. This function is called after a card removal is detected.

Use the callback that is set by the `CTRDG_SetPulledOutCallback` and `CTRDG_IsPulledOut` functions to detect a Game Pak removal.

The stop notification that is sent to ARM7 is sent internally by a PXI signal. Do not call this function when PXI interrupts are prohibited.

## Arguments

None.

## Return Values

None.

## See Also

`CTRDG_Init`, `CTRDG_SetPulledOutCallback`, `CTRDG_IsPulledOut`, `CTRDG_IsExisting`

## Revision History

09/15/2004 Initial version