# CARDBackupType

## C Specification

      #include <nitro/card.h>
      typedef enum {

      CARD_BACKUP_TYPE_EEPROM_4KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 9, 0),
      CARD_BACKUP_TYPE_EEPROM_64KBITS = CARD_BACKUP_TYPE_DEFINE(EEPROM, 13, 0),
      CARD_BACKUP_TYPE_FLASH_2MBITS = CARD_BACKUP_TYPE_DEFINE(FLASH, 18, 0),
      CARD_BACKUP_TYPE_NOT_USE = 0

      } CARDBackupType;

## Description

Indicates the enumerated constants that identifies the backup device that is mounted in a NITRO-CARD.

## See Also

`CARD_IdentifyBackup, CARD_GetCurrentBackupType`

## Revision History

09/09/2004 Deleted `CARD_BACKUP_TYPE_EEPROM_512KBITS` and `CARD_BACKUP_TYPE_EEPROM_1MBITS`
08/23/2004 Changed the enumeration type format and added `CARD_BACKUP_TYPE_FLASH_2MBITS`
07/05/2004 Initial version