# NNS_G2dLoadPalette

## C Specification

      #include <nnsys/g2d/g2d_Image.h>

      void NNS_G2dLoadPalette(
      const NNSG2dPaletteData*            pSrcData,
      u32                                 addr,
      NNS_G2D_VRAM_TYPE           type,
      NNSG2dImagePaletteProxy*    pPltProxy );

## Arguments

pSrcData | [IN] Input image data source
addr | [IN] Load destination address
`type` | [IN] VRAM type to use (3D, 2D-Main, or 2D-Sub)
pPltProxy | [OUT] Image palette proxy that stores the load result

## Return Values

None.

## Description

Loads the image palette data to the hardware and sets the load results and the image format to the image palette proxy.

## See Also

None.

## Revision History

05/28/2004 Initial version.