# NNS_G3dGlbGetWV

## C Specification

      #include <nnsys/g3d/glbstate.h>

      const MtxFx43* NNS_G3dGlbGetSrtCameraMtx( void );
      const MtxFx43* NNS_G3dGlbGetWV(void);

## Arguments

None.

## Return Values

Returns the pointer to the matrix multiplied by the `BaseSRT` matrix in the camera matrix.

## Description

This function gets the pointer to the matrix multiplied by the `BaseSRT` matrix in the camera matrix that is set to the global state kept in the G3D library. When the matrix was not calculated by multiplying with the `BaseSRT` matrix, the matrix is requested and then the pointer to the matrix is returned. At this time, the inverse matrix that is returned by the `NNS_G3dGlbGetInvWV` function function is also calculated.

## See Also

`NNS_G3dGlbGetInvWV`

## Revision History

10/13/2004 Removed `NNS_G3dGlbGetSrtCameraMtx` from the title but left it in the C Specification section.
08/02/2004 Initial version.