# GX_SetBankForTexPltt

## C Specification

  `#include <nitro/gx/gx_vramcnt.h>`
  `void GX_SetBankForTexPltt(GXVRamTexPltt texPltt);`

## Arguments

texPltt | Specifies a VRAM bank to allocate to the texture palette

## Return Values

None.

## Description

This function allocates the specified VRAM bank to the texture palette. If the specified VRAM bank is either disabled or allocated to LCDC, this allocates the VRAM bank to the texture palette.

`GX_VRAM_TEXPLTT_NONE` | A VRAM bank is not allocated to the texture palette.
`GX_VRAM_TEXPLTT_0_F` | Slot 0 of the texture palette is reserved. VRAM-F is allocated.
`GX_VRAM_TEXPLTT_0_G` | Slot 0 of the texture palette is reserved. VRAM-G is allocated.
`GX_VRAM_TEXPLTT_01_FG` | Slot 0.1 of the texture palette is reserved. VRAM-F and -G are allocated.
`GX_VRAM_TEXPLTT_0123_E` | Slots 0, 1, 2, and 3 of the texture palette are reserved. VRAM-E is allocated.
`GX_VRAM_TEXPLTT_01234_EF` | Slots 0, 1, 2, 3, and 4 of the texture palette are reserved. VRAM-E and -F are allocated.
`GX_VRAM_TEXPLTT_012345_EFG` | Slots 0, 1, 2, 3, 4, and 5 of the texture palette are reserved. VRAM-E, -F, and -G are allocated.

The following is the type definition for `GXVRamTexPltt` types.

    typedef enum
    {
    GX_VRAM_TEXPLTT_NONE     = 0x0000,
    GX_VRAM_TEXPLTT_0_F      = GX_VRAM_F,              // TexturePltt 0
    GX_VRAM_TEXPLTT_0_G      = GX_VRAM_G,              // TexturePltt 0
    GX_VRAM_TEXPLTT_01_FG    = GX_VRAM_F | GX_VRAM_G,  // TexturePltt 01
    GX_VRAM_TEXPLTT_0123_E   = GX_VRAM_E,              // TexturePltt 0-3
    GX_VRAM_TEXPLTT_01234_EF = GX_VRAM_E | GX_VRAM_F,  // TexturePltt 0-3,4
    GX_VRAM_TEXPLTT_012345_EFG = GX_VRAM_E | GX_VRAM_F | GX_VRAM_G  // TexturePltt 0-3,45
    }
    GXVRamTexPltt;

## See Also

`GX_GetBankForTexPltt`, `GX_ResetBankForTexPltt`, `GX_DisableBankForTexPltt`, `GX_GetSizeOfTexPltt`

## Revision History

01/19/2004 Initial version