# MB_DisconnectChild

## C Specification

  `#include <nitro/mb.h>`
  `void MB_DisconnectChild( u16 aid );
  `

## Arguments

aid | The `aid` of the child to disconnect.

## Return Values

None.

## Description

This function operates from the parent side, forcibly disconnecting a child from the MB parent. This function immediately removes control of the DS device as a multiboot child and begins the wireless disconnection process. This function does not return a callback at the end of the wireless disconnection.

## See Also

## Revision History

11/10/2004 Initial version.