# GX_GetVCountEqVal

## C Specification

      #include <nitro/gx/gx.h>

      s32 GX_GetVCountEqVal(void);

## Arguments

None.

## Return Values

The value set as equal to the V-counter

## Description

This function configures the parity value that will be equal to the V-counter. The value must be an integer between 0 and 262.

There is no need to manipulate the value set as equal to the V-counter, except when operating the VCOUNT interrupt directly without using the VAlarm provided in SDK.

`GX_GetVCountEqVal` is also defined with the different name of `GX_GetVCounterEqVal`.

## See Also

`GX_SetVCountEqVal`, `GX_IsVCountEq`, `GX_VCountEqIntr`

## Revision History

10/19/2004 Initial version.