# G2S_GetBG1ScrPtr

## C Specification

      #include <nitro/gx/g2.h>

      void *G2S_GetBG1ScrPtr();

## Arguments

None.

## Return Values

A pointer to the region where BG1 screen data is stored.

## Description

This function returns a pointer to the region where sub 2D engine BG1 screen data is stored. The return values are as follows:

> The value at the end of the enumerator type value name `GXBGScrBase` that is specified by `HW_DB_BG_VRAM` + (`G2S_SetBG1Control`).

## See Also

`G2S_SetBG1Control, G2S_SetBG1Priority, G2S_BG1Mosaic, G2S_GetBG1CharPtr, G2S_SetBG1Offset`

## Revision History

02/09/2004 Initial version.

CONFIDENTIAL