# CARD_IsBackupFlash

## C Specification

  `#include <nitro/card.h>`
  `static inline BOOL CARD_IsBackupFlash(void);`

## Arguments

None

## Return Values

Returns TRUE if the designated backup device is FLASH, and FALSE if it is not.

## Description

This function determines whether the type of the backup device designated by the `CARD_IdentifyBackup` function is FLASH.

## See Also

`CARD_IdentifyBackup, CARD_ReadFlash, CARD_WriteFlash`

## Revision History

08/23/2004 Revised the links due to changes to the function
08/18/2004 Initial Version

CONFIDENTIAL