# G3X_GetBoxTestResult

## C Specification

      #include <nitro/gx/g3x.h>

      int G3X_GetBoxTestResult(s32 * in);

## Arguments

in | Pointer to variable storing the test results

## Return Values

Whether the test has completed (0) or is still execution (not 0).

## Description

If the return value is 0, the test results are in `*``in`.

- A value other than 0 indicates that part or all of the box is in the view volume.
- A value of 0 indicates that the entire box is outside the view volume.

If the return value is not 0, the test is still executing.

## See Also

G3_BoxTest

## Revision History

01/19/2004 Initial version

CONFIDENTIAL