# PM_GetLCDPower

## C Specification

      #include <nitro/spi.h>

      PMLCDPower PM_GetLCDPower( void );

## Arguments

None.

## Return Values

This function returns the LCD switch state using the following values: PM_LCD_POWER_ON LCD is switched ON PM_LCD_POWER_OFF LCD is switched OFF

## Description

This function gets the LCD switch state.

## Internal Operation

This function is accessed by the GX_POWCNT register.

## See Also

`PM_Init`, `PM_SetLCDPower`

## Revision History

08/07/2004 Initial version.

CONFIDENTIAL