# PADi_ClearIrq

## C Specification

  `#include <nitro/pad/pad.h>`
  `void PADi_ClearIrq( void );`

## Arguments

None.

## Return Values

None.

## Description

This function prohibits interrupts corresponding to key input. This function zero-clears the IO register `REG_KEYCNT` (Key Control).

## See Also

`PAD_Read, PADi_SetIrq`

## Revision History

03/08/2005 Standardized the Japanese term for "interrupt"
12/01/2003 Initial version

CONFIDENTIAL