# MI_WriteByte

## C Specification

  `#include <nitro/mi.h>`
  `void MI_WriteByte( void* address, u8 data);`

## Arguments

address | Address for writing byte data (pointer)
data | The data to write.

## Return Values

None.

## Description

This function writes byte data to the address specified by a void typed pointer. Internally, it accesses memory as u16 data. Therefore at assembler level, byte access instructions such as `strb/ldrb` will not be generated.

## See Also

MI_ReadByte

## Revision History

03/30/2004 Initial version.

CONFIDENTIAL