# G2S_GetBG0ScrPtr

## C Specification

      #include <nitro/gx/g2.h>

      void *G2S_GetBG0ScrPtr();

## Arguments

None.

## Return Values

The pointer to the region storing the BG0 screen.

## Description

This function returns a pointer to the region where sub 2D engine BG0 screen data is stored. The return values are as follows:

> The value at the end of the enumerator type value name `GXBGScrBase` that is specified by `HW_DB_BG_VRAM` + (`G2S_SetBG0Control`).

## See Also

`G2S_SetBG0Control, G2S_SetBG0Priority, G2S_BG0Mosaic, G2S_GetBG0CharPtr, G2S_SetBG0Offset`

## Revision History

02/09/2004 Initial version.

CONFIDENTIAL