G3*_MultMatrix33

# G3*_MultTransMtx33

## Syntax

      #include <nitro/gx/g3imm.h>
      #include <nitro/gx/g3b.h>
      #include <nitro/gx/g3c.h>

      void G3_MultTransMtx33(const MtxFx33* m);

      // Below are APIs for creating the display list (command list)
      void G3B_MultTransMtx33(GXDLInfo* info, const MtxFx33* mtx, const VECFx32* vec);
      void G3C_MultTransMtx33(GXDLInfo* info, const MtxFx33* mtx, const VECFx32* vec);
      void G3BS_MultTransMtx33(GXDLInfo* info, const MtxFx33* mtx, const VECFx32* vec);
      void G3CS_MultTransMtx33(GXDLInfo* info, const MtxFx33* mtx, const VECFx32* vec);

## Arguments

info | Command List Information.
mtx | Pointer to the matrix to be multiplied
vec | Pointer to the distance vector to translate

## Return Values

None.

## Description

The current matrix is multiplied on the left by a 4x3 matrix. This process is equivalent to multiplying the current matrix by both a translation matrix and a 3x3 matrix. Each element of the matrix is a signed fixed-point number (sign + 19-bit integer + 12-bit decimal). If the current matrix is `C`, then the new matrix, `Cnew`, is in the format shown below.

## See Also

`G3*_MultMtx43, G3*_MultMtx33, G3*_Translate`

## Revision History

2004/08/02 Initial version.

CONFIDENTIAL