# MI_StopAllNDma

## Syntax

  `#include <twl/mi.h>`
  `void MI_StopAllNDma( void );`

## Arguments

None.

## Return Values

None.

## Description

Stops all new DMA channels. This function does not stop the legacy DMA that has been carried over from the NITRO hardware.

This function calls the `MI_StopNDma` function for new DMA channels 0-3.

## See Also

`MI_StopNDma
`

## Revision History

2008/09/11 Initial version.

CONFIDENTIAL