SCFG_GetSystemRomType

# SCFG_IsClockSuppliedToDSP

## Syntax

      #include <twl/scfg.h>

      static inline BOOL SCFG_IsClockSuppliedToDSP( void );

## Arguments

None.

## Return Values

If `TRUE`, a clock is being supplied to the DSP block.
If `FALSE`, a clock is not being supplied.

## Description

Gets the clock supply setting for the DSP block.

Note: Use this function when running on TWL hardware.

Because NITRO hardware does not include an SCFG block, this function is not expected to be invoked on NITRO hardware.

## See Also

SCFG Overview
`SCFG_SupplyClockToDSP`

## Revision History

2007/10/03 Initial version.

CONFIDENTIAL