# GXS_HBlankOBJProc

## Syntax

  `#include <nitro/gx/gx.h>`
  `void GXS_HBlankOBJProc(BOOL proc);`

## Arguments

blank | Flag that sets whether the OBJ rendering process occurs during H-Blank

## Return Values

None.

## Description

When the argument is `TRUE`, the OBJ rendering process occurs only during the display period and not during the H-Blank period. In this case, the maximum OBJ display performance cannot be used. When the argument is `FALSE`, the OBJ rendering process is performed for all H-Line periods (including H-Blank periods).

## See Also

## Revision History

2004/02/09 Initial version.

CONFIDENTIAL