# G3X_SetEdgeColorTable

## Syntax

  `#include <nitro/gx/g3x.h>`
  `void G3X_SetEdgeColorTable(const GXRgb * rgb_8);`

## Arguments

rgb_8 | Pointer to the beginning of the color data array set in the edge color table

## Return Values

None.

## Description

This function sets the edge color table. Data from `rgb_8[0]` to `rgb_8[7]` is transferred to the edge color table.

## See Also

G3X_EdgeMarking

## Revision History

2004/01/19 Initial version.

CONFIDENTIAL