# GX_EndLoadTex

## Syntax

  `#include <nitro/gx/gx_load.h>`
  `void GX_EndLoadTex(void);`

## Arguments

None.

## Return Values

None.

## Description

This function is called after transferring texture images to the texture image slot. Internally, it restores to the texture image slot the VRAM bank that was allocated to LCDC by `GX_BeginLoadTex`.

## See Also

`GX_BeginLoadTex, GX_EndLoadTex`

## Revision History

2004/02/09

- Revised and expanded the description.

2004/01/19 Initial version.

CONFIDENTIAL