# MI_WriteByte

## Syntax

  `#include <nitro/mi.h>`
  `void MI_WriteByte( void* address, u8 data )`

## Arguments

address | Address for writing byte data (pointer)
data | The data to write.

## Return Values

None.

## Description

This function writes byte data to the address specified by a `void`-type pointer.

This function ensures compatibility with previous versions. Currently, this is just an inline function that writes data by treating address as a u8 pointer.

## See Also

`MI_ReadByte`

## Revision History

2008/07/09 Revised the reference to match the current specifications.
2004/03/30 Initial version.

CONFIDENTIAL