# MTX_Copy33To44

## Syntax

      #include <nitro/fx/fx_mtx33.h>

      void MTX_Copy33To44(const MtxFx33 * pSrc, MtxFx44 * pDst);

## Arguments

pSrc | Pointer to a 3x3 matrix.
pDst | Pointer to a 4x4 matrix.

## Return Values

None.

## Description

This function copies a 3x3 matrix to a 4x4 matrix. The element in the 4th row of the 4th column of the 4x4 matrix is set to `FX32_ONE`; all other elements in the 4th row and 4th column are set to 0.

## See Also

`MtxFx33, MtxFx44`

## Revision History

2004/01/19 Initial version.

CONFIDENTIAL