# SCFG_ReleaseResetDSP

## Syntax

      #include <twl/scfg.h>

      static inline void SCFG_ReleaseResetDSP( void );

## Arguments

None.

## Return Values

None.

## Description

Cancels the DSP block reset.

Note: Use this function when running on TWL hardware.

Because NITRO hardware does not include an SCFG block, this function is not expected to be called on NITRO hardware.

## See Also

SCFG Overview
`SCFG_ResetDSP`
`SCFG_IsDSPReset`

## Revision History

2007/10/03 Initial version.

CONFIDENTIAL