# G2*_GetBG1Control

## Syntax

  `#include <nitro/gx/gx_bgcnt.h>`

      static inline GXBg01Control G2_GetBG1Control( void );
      static inline GXBg01Control G2S_GetBG1Control( void );

## Arguments

None.

## Return Values

The display settings for BG1.

## Description

Gets the display settings for BG1 as the structure `GXBg01Control`. See the `G2_SetBG1Control` function for more information on each member.
Use the `G2_GetBG1Control` function to get the settings for the main 2D engine and the `G2S_GetBG1Control` function to get the settings for the sub 2D engine. The following is the definition for `GXBg01Control`:

    typedef union
    {
        u16 raw;
        struct
        {
            u16 priority    :2;
            u16 charBase:4;
            u16 mosaic:1;
            u16 colorMode:1;
            u16 screenBase:5;
            u16 bgExtPltt:1;
            u16 screenSize:2;
        };
    }
    GXBg01Control;

## See Also

`G2_SetBG1Control
G2S_SetBG1Control`

## Revision History

2004/12/24 Initial version.

CONFIDENTIAL