# WFS_GetClientReadProgress

## Syntax

  `#include <nitro/wfs.h>`
  `void WFS_GetClientReadProgress(WFSClientContext *context, int *current, int *total);`

## Arguments

context | Pointer to the `WFSClientContext` structure.
current | Pointer to the int variable used to retrieve the number of packets already received
total | Pointer to the int variable used to retrieve the total number of packets expected to be received

## Return Values

None.

## Description

Gets the current status of a ROM image read request that was issued using `WFS_RequestClientRead`. Progress status can be retrieved in the format (number of packets already received) / (total number of packets expected).

## See Also

`WFS_RequestClientRead`

## Revision History

2007/06/06 Initial version.

CONFIDENTIAL