# MB_CommIsBootable

## Syntax

  `#include <nitro/mb.h>`
  `BOOL MB_CommIsBootable( u16 child_aid );`

## Arguments

child_aid | The aid that specifies the child that checks the child state

## Return Values

Returns `TRUE` when in a state where the specified child is bootable. Otherwise returns `FALSE`.

## Description

Determines whether or not the system is currently in a state in which the specified child is bootable as a multiboot child.

## See Also

`MB_CommGetParentState`, `MB_CommBootRequest`

## Revision History

2004/10/05 Initial version.

CONFIDENTIAL