# OS_GetITCMAddress

## Syntax

      #include <nitro/os.h>

      u32 OS_GetITCMAddress( void );

## Arguments

None.

## Return Values

The instruction TCM base address.

## Description

Gets the instruction TCM base address This address is always 0x01FF8000 (constant HW_ITCM).

## See Also

`OS_GetDTCMAddress
`

## Revision History

2005/02/17 Revised description of return value
2004/06/11 Added description
2004/02/10 Initial version

CONFIDENTIAL