CameraWhiteBalanece

# CAMERAWhiteBalance

## 定義

  `#include <twl/camera.h>`

      typedef enum
      {
          CAMERA_WHITE_BALANCE_AUTO,

          CAMERA_WHITE_BALANCE_3200K,
          CAMERA_WHITE_BALANCE_4150K,
          CAMERA_WHITE_BALANCE_5200K,
          CAMERA_WHITE_BALANCE_6000K,
          CAMERA_WHITE_BALANCE_7000K,

          CAMERA_WHITE_BALANCE_MAX,

          // alias
          CAMERA_WHITE_BALANCE_NORMAL                     = CAMERA_WHITE_BALANCE_AUTO,
          CAMERA_WHITE_BALANCE_TUNGSTEN                   = CAMERA_WHITE_BALANCE_3200K,
          CAMERA_WHITE_BALANCE_WHITE_FLUORESCENT_LIGHT    = CAMERA_WHITE_BALANCE_4150K,
          CAMERA_WHITE_BALANCE_DAYLIGHT                   = CAMERA_WHITE_BALANCE_5200K,
          CAMERA_WHITE_BALANCE_CLOUDY                     = CAMERA_WHITE_BALANCE_6000K,
          CAMERA_WHITE_BALANCE_HORIZON                    = CAMERA_WHITE_BALANCE_6000K,
          CAMERA_WHITE_BALANCE_SHADE                      = CAMERA_WHITE_BALANCE_7000K
      }
      CAMERAWhiteBalance;

## 要素

CAMERA_WHITE_BALANCE_TUNGSTEN | 3200K　（白熱電球）
CAMERA_WHITE_BALANCE_WHITE_FLUORESCENT_LIGHT | 4150K　（白色蛍光灯）
CAMERA_WHITE_BALANCE_DAYLIGHT | 5200K　（太陽光）
CAMERA_WHITE_BALANCE_CLOUDY | 6000K　（くもり）
CAMERA_WHITE_BALANCE_HORIZON | 6000K　（夕焼け）
CAMERA_WHITE_BALANCE_SHADE | 7000K　（日陰）
CAMERA_WHITE_BALANCE_NORMAL | オート

## 説明

カメラのホワイトバランスを指定するために使用する列挙型です。

## 履歴

2008/03/13 定義の変更
2007/11/12 初版