# NNS_G3dGeIsBufferOK

## Syntax

      #include <nnsys/g3d/gecom.h>

      BOOL
      NNS_G3dGeIsBufferOK(
          u32 numWord
      );

## Arguments

numWord | The number of pieces of data that you wish to append to the command buffer.

## Return Values

Returns `TRUE` if `numWord` pieces of data can be added to the geometry command buffer.

## Description

This function checks whether a `numWord` quantity of data can be buffered to the geometry command buffer. Always returns `FALSE` when the geometry command buffer is not configured.

## See Also

## Revision History

2004/10/15 Added description.
2004/08/02 Initial version.

CONFIDENTIAL