# NNS_SndPlayerGetSeqType

## Syntax

      #include <nnsys/snd.h>

      NNSSndPlayerSeqType NNS_SndPlayerGetSeqType(
              NNSSndHandle* handle );

## Arguments

`handle` | The sound handle pointer.

## Return Values

Returns the sequence data type.

## Description

Gets the sequence data type.

This function gets the sequence data type of the sequence that is bound to the sound handle `handle`. If the sound handle is invalid, `NNS_SND_PLAYER_SEQ_TYPE_INVALID` is returned.

The information that can be obtained is based on the value that is set by the `NNS_SndPlayerSetSeqNo` function or the `NNS_SndPlayerSetSeqArcNo` function.

TABLE: NNSSndPlayerSeqType

Label | Value | Description
--- | --- | ---
NNS_SND_PLAYER_SEQ_TYPE_INVALID | 0 | The handle is invalid, or the sequence data number has not yet been set
NNS_SND_PLAYER_SEQ_TYPE_SEQ | 1 | The sequence data
NNS_SND_PLAYER_SEQ_TYPE_SEQARC | 2 | The sequence archive

## See Also

`NNS_SndPlayerSetSeqNo`, `NNS_SndPlayerSetSeqArcNo`

## Revision History

2004/06/01 Initial version.

CONFIDENTIAL